[image: A logo with a sun and mountains in the background

AI-generated content may be incorrect.]


	[bookmark: _Hlk210220243]CENTERVILLE CITY LANDSCAPING CHECKLIST

	Landscaping– Completeness Checklist 
The following application, information, fees, and documentation is required for a landscaping plan completeness review.

Project Name: 
Date: 
[image: Checkmark with solid fill][image: Question mark with solid fill]X –



	Landscaping Plan Required Items: 
	
	

	Landscaping and plant materials;

	12.51.040
	

	Location, spacing, and number of existing and proposed plantings;

	12.51.040
	

	Mature tree canopy line;

	12.51.040
	

	Tree and plant list, including sizes and totals;

	12.51.040
	

	Treatment of ground surfaces;
	12.51.040
	

	Use of non live landscaping materials such as hard surface improvements or artificial landscaping identified;
	12.51.040
	

	Irrigation or watering plan;
	12.51.040
	

	Such other information as may be needed to demonstrate compliance with the provisions of this Chapter
	12.51.040
	

	Landscape Architect Approval. A landscape plan for a site of one acre or more, or any amendment thereto, shall be signed by and bear the seal of a Utah licensed landscape architect licensed under the Landscape Architects Licensing Act, as set forth in Utah Code Ann. §§ 58-53-101, et seq.
	12.51.040
	

	Landscape designs should include plantings that provide shade for structures, outdoor recreational areas, and parking areas.
	12.51.060
	

	Required landscaping areas shall include live plant material at least to the following extent:
· Perimeter and internal landscaping: 50% of perimeter and internal landscaped area shall include live plant material
· Buffer landscaping between residential and non-residential development: 50% of buffer landscaped area shall include live plant material
· The use of lawn and turf for live plant material is restricted and subject to CMC 12.51.065 
	12.51.070
	

	Excluding parkstrips, non-live landscaping or hardscaping materials may consist of hard surface improvements such as decorative boulders, planters, benches, sculptures, water features, or materials such as wood chips, bark, stone, decorative gravel, mulch, or other similar materials. 
	12.51.070
	

	Non-live landscaping or hardscaping materials shall not be deemed to include artificial plants or landscaping. Artificial plants and landscaping, such as artificial or man-made shrubs, trees or other similar vegetation or landscaping material, may be utilized in a landscaping plan. No artificial plants or landscaping shall qualify or be used to meet the minimum landscaping requirements 
	12.51.070
	

	Decorative paving materials may include bricks, pavers, flagstones, and decoratively textured or colored concrete.
	12.51.070
	

	Deciduous trees are the preferred tree type. Coniferous trees are generally discouraged but may be used for screening objects such as dumpsters and mechanical enclosures. 

	12.51.070
	

	One tree shall be planted for every 500 square feet of landscaped area not including any requirement for plantings for buffers and architectural barriers
	12.51.070
	

	Trees may be substituted by shrubs at a ratio of 10 shrubs to one tree. Not more than 25% of required trees may be substituted by shrubs
	12.51.070
	

	Total landscaped areas for projects should have at least 35% plant foliage coverage at the plant's maturity. Annual flowers and other annual plants and flower bulbs are generally not used to calculate the 35% recommended plant foliage coverage. 
	12.51.075
	

	Plant Material Standards
	
	

	Plants used for landscaping shall:
· Be drought tolerant;
· Have non-invasive growth habits;
· Have low maintenance characteristics; and
· Be commercially available.
	12.51.080
	

	The minimum size of trees and plants installed to meet the requirements to this Chapter shall be as follows:
· Deciduous trees: 2 inch caliper (diameter) measured at 12 inches above the tree base.
· Coniferous trees: 6 feet high.
· Shrubs: 18 inches high.
	12.51.080
	

	Box Elder, Salix and Poplar trees shall be prohibited within 25 feet of a public right-of-way and public utility easements.
	12.51.080
	

	Elm trees shall be prohibited.
	
	

	Shrub size shall be a #5 container with a spread of 18 to 24 inches when installed
	12.51.070
	

	Lawn and Turf Restrictions
	
	

	Parkstrips - All Zones. No lawn or turf shall be permitted in any parkstrip area in any zone within the City. 
	12.51.065
	

	Narrow Areas - All Zones. No lawn or turf shall be permitted in any areas less than 8 feet wide in any zone within the City.
	12.51.065
	

	Front and Side Yards - Single-Family Residential Lots or Parcels. Lawn and turf shall not exceed 35% of the front and side yard landscaped areas of single-family residential lots or parcels; provided, such restrictions shall not apply to small single-family residential lots or parcels with less than 250 square feet of landscaped area.
	12.51.065
	

	Total Landscaped Areas - Commercial, Industrial, Public Facility, and Multifamily Zones. Lawn and turf shall not exceed 15% of the total landscaped areas of commercial, industrial, public facility, mixed use, specialty, overlay, multifamily, or any other non-single-family residential properties and projects; provided, such restrictions shall not apply to approved active recreational areas that meet State and local water conservancy district design and landscaped standards.
	12.51.065
	

	To avoid damage to public rights-of-way, unless otherwise approved, trees shall not be planted in parkstrips and should be at least 7 feet from the edge of a sidewalk.
	12.51.070
	

	Drainage
	
	

	Landscaped detention or retention areas, plant material should be compatible with the use
	12.51.060
	

	Detention or retention area side slopes should not exceed a one to three (1:3) vertical to horizontal slope unless fenced to prohibit public access. 

	12.51.060
	

	Detention or retention basins should be designed as an integral part of the landscape theme and not appear as a ditch or pit.
	12.51.060
	

	Artificial plants and landscaping shall not be permitted in storm water detention or retention areas.

	12.51.060
	

	Building Foundations 
	
	

	Landscaping should be provided along building foundations in locations visible to the general public.

	12.51.060
	

	Landscaped areas shall be located:
· Adjacent to building elevations which form major public views of a project from adjacent streets and property, and to users of the project
· Between buildings or portions of buildings, in parking lots, and in any plaza or courtyard
	12.51.070
	

	At least 50% of the building frontage shall be landscaped
	12.51.070
	

	The minimum width of the landscaped area shall be three feet, excluding any vehicle overhang from an adjacent parking area
	12.51.070
	

	Ground Cover
	
	

	A mixture of vegetative ground cover and hardscape may be used along public rights-of-way and in required front yard landscape areas
	12.51.060
	

	Rock, mulch, or other similar materials used in planting beds or other areas should have a depth of at least three to four inches to prevent weed growth and retain soil moisture and should be permeable to air and water. The use of rock, mulch, or other materials in the parkstrip is restricted by City ordinances, including, but not limited to CMC 11.02.020 (Parkstrip Landscaping and Hardscaping).
	12.51.075
	

	Water Usage
	
	

	Drought resistant shrubs and trees, as established by typical planting standards for the Western United States region.
	12.51.060
	

	Ninety percent (90%) of all plant materials should be drought tolerant and water-efficient plantings, as listed or depicted in various water conservation demonstration gardens in Utah or as recommended by a landscape architect. 
	12.51.075
	

	Water-efficient or water-wise landscaping, as defined in Utah Code 10-20-619, should be used wherever possible
	12.51.060
	

	Irrigation systems shall be automatic and shall include rain delay sensors (e.g. WaterSense labeled smart irrigation controlled systems)
	12.51.070
	

	Irrigation systems should be designed with water-efficient controllers, valves, drip emitters, and bubblers that provide the minimum necessary amount of water to ideally sustain the landscape plantings (e.g. WaterSense labeled smart irrigation controlled systems).
	12.51.075
	

	Drip irrigation systems should be used for all non-turf landscaped areas.
	12.51.075
	

	Planting areas should be irrigated with low-volume drip irrigation systems. Low-volume drip emitters should be rated at 5 gallons or less. Micro-spray emitters, bubblers, and soaker hoses are not considered low-volume drip irrigation. 
	12.51.075
	

	Overhead sprinklers (generally used for lawn, turf, or other landscaping) should not be on the same irrigation valve or zone as drip irrigation (generally used for plants and shrubs).
	12.51.075
	

	Drip irrigation systems should be installed with filter and pressure regulators. 

	12.51.075
	

	No Use of Culinary Water for Irrigation. Unless otherwise provided, such as areas not serviced by secondary water, the City prohibits the use of culinary water to water landscaped areas and all landscaped areas shall be watered with secondary irrigation water service.
	12.51.075
	

	Watering Times. Irrigation operation and watering shall only be permitted between the hours of 6 p.m. to 10 a.m. to reduce loss from wind and minimize evaporation or as restricted by other local, special service district, county, or state regulations, including, but not limited to CMC 9.02.210 (Sprinklers).
	12.51.075
	

	Artificial Landscape Standards 
	
	

	Parrish Lane Gateway Area: 
Artificial landscaping shall not be allowed. 
	12.51.082
	

	South Main Street Commercial Area:
Artificial landscaping shall be prohibited within the following Subdistricts of the SMSC Overlay Zone: the North Gateway/Mixed-Use Subdistrict, the Traditional Main Street Subdistrict and the City Center Main Street Subdistrict. 

Artificial landscaping shall be permitted the following Subdistricts of the South Main Street Corridor: the Civic/Cultural Subdistrict, the Residential Boulevard Subdistrict, and the Pages Lane Mixed Use Subdistrict, subject to the following requirements and standards: 
· Artificial plants shall mimic the look, texture and color of the genus or species that it is intended to represent, including branches, stems, leaves, trunk and canopy size, as applicable
· Artificial plants shall not be illuminated or outlined with attached external illumination devices
· Artificial plants shall comply with all applicable building, electrical and safety codes, including wind and snow load requirements for Centerville City and shall not exceed a height of 25 feet.
· Artificial plants and landscaping may only be used in the on-site landscaped areas. 
· No artificial plants or landscaping shall be permitted in the public right-of-way or to satisfy any street tree requirement. No artificial plants or landscaping shall be permitted in any required landscaped buffer, storm water detention, parking lot, public street frontage or parkstrip area.
· No artificial plants or landscaping shall be installed in such a way as to hang over or encroach onto adjacent property or public rights-of-way. 
· Artificial plants shall be set back a minimum distance of three feet from any property line and artificial plants that are taller than three feet shall be set back a minimum distance from any property line equal to at least the height of the artificial plant. 
· Artificial plants and landscaping shall meet the sight triangle for any intersection area of 30 feet
· The total amount of artificial plants and landscaping on any given site shall not exceed 5% of the total landscaped area on the site

	12.51.082
	

	Frontage Road Area: 
Artificial landscaping shall be permitted in accordance with the terms and conditions of this Chapter within the Frontage Road Area, subject to the following requirements and standards:

· Artificial plants shall mimic the look and texture of the genus or species that it is intended to represent, including branches, stems, leaves, trunk and canopy size, as applicable. 
· Artificial plants shall not be illuminated or outlined with attached external illumination devices
· Artificial plants shall comply with all applicable building, electrical and safety codes, including wind and snow load requirements for Centerville City and shall not exceed a height of 25 feet.
· Artificial plants and landscaping may only be used in the on-site landscaped areas. 
· No artificial plants or landscaping shall be permitted in the public right-of-way or to satisfy any street tree requirement. 
· No artificial plants or landscaping shall be permitted in any required landscaped buffer, storm water detention, parking lot, public street frontage or parkstrip area.
· No artificial plants or landscaping shall be installed in such a way as to hang over or encroach onto adjacent property or public rights-of-way.
· Artificial plants shall be set back a minimum distance of 10 feet from any property line. 
· Artificial plants and landscaping shall meet the sight triangle for any intersection area of 30 feet
· The total amount of artificial plants and landscaping on any given site shall not exceed 25% of the total landscaped area on the site
	12.51.082
	

	All Other Areas: 
Artificial landscaping shall be permitted subject to the following requirements and standards:
· Artificial plants shall mimic the look, texture and color of the genus or species that it is intended to represent, including branches, stems, leaves, trunk and canopy size, as applicable.
· Artificial plants shall not be illuminated or outlined with attached external illumination devices
· Artificial plants shall comply with all applicable building, electrical and safety codes, including wind and snow load requirements for Centerville City and shall not exceed a height of 25 feet.
· Artificial plants and landscaping may only be used in the on site landscaped areas. 
· No artificial plants or landscaping shall be permitted in the public right-of-way or to satisfy any street tree requirement. No artificial plants or landscaping shall be permitted in any required landscaped buffer, storm water detention, parking lot, public street frontage or parkstrip area.
· Artificial plants shall be set back a minimum distance of t3 feet from any property line and artificial plants that are taller than 3 feet shall be set back a minimum distance from any property equal to at least the height of the artificial plant. 
· Artificial plants and landscaping shall meet the sight triangle for any intersection area of 30 feet
· The total amount of artificial plants and landscaping on any given site shall not exceed 10% of the total landscaped area on the site
· 
	12.51.082
	

	Buffers
	
	

	Landscaped buffers shall be required along side and rear property boundaries of commercial or industrial property or projects which abut a residential zone.

For commercial, industrial, or other non-residential property (source zone) abutting a residential zone, the minimum landscaped buffer depth shall be as follows:
· In medium intensity (M) source zones: 15 feet
· In high intensity (H) and very high intensity (VH) source zones: 30 feet
	12.51.070
	

	Landscaped buffers shall also be required along side and rear property boundaries of any Residential High (R-H) zoned property or projects which abut Residential Low (R-L) zoned property.

For high intensity residential (R-H) property (source zone) abutting a low intensity residential zone (R-L), the minimum landscaped buffer depth shall be as follows:
· In high intensity (H) source zones meeting low intensity (L) zones: 25 feet
	12.51.070
	

	An architectural buffer at least six feet in height shall be provided within the buffer zone. 
	12.51.070
	

	Buffer may consist of either a block or concrete wall, fencing, or live plants 
	12.51.070
	

	An architectural buffer consists of solid fencing or a wall, evergreen landscaping anticipated to grow to more than six feet in height shall be provided at distances sufficient to provide a visual and noise reducing barrier. Such landscaping shall consist of at least one tree for every 20 feet of fencing.
	12.51.070
	

	If an architectural buffer does not consist of solid fencing or a wall, a sufficient quantity of evergreen trees and shrubs shall be provided which are reasonably anticipated to grow to approximately six feet in height to produce a solid landscape screen through all seasons of the year.
	12.51.070
	

	Architectural buffers on corner lots shall be modified to comply with required sight and visibility standards ( 30 ft sight triangle must be shown for all corner lots). 
	12.51.070
	

	Artificial plants and landscaping shall not be permitted in the required landscaped buffer areas.
	12.51.070
	

	Screening
	
	

	Trash Receptacles 
Shall be screened from view by a wall or fence which:
· Is at least six feet in height
· Provides complete visual screening of the receptacle
· Is compatible in material and color with the main building on the lot or parcel.
	12.51.110
	

	Outdoor Storage Areas 
Shall be screened from view by an opaque fence or wall. 
Non-opaque fencing, such as powder or vinyl coated chain-link, may be used to satisfy this requirement in industrial zones if vinyl slats are inserted into the fence.
	12.51.110
	

	Service and Loading Areas
Shall be screened from public view
	12.51.110
	

	Ground-Mounted Utility Boxes, Meters and Mechanical Equipment
Shall be screened from public view by landscaping or architectural elements compatible in material and color with the main building on the lot or parcel. 

This requirement shall not apply to:
· Rear and rear side yard locations adjacent to other service or mechanical areas not adjacent to a public street; and 
· Development in agricultural and R-L Zones.

	12.51.110
	

	Roof-Mounted Mechanical Equipment
Shall be concealed by material which is consistent with building design and is equal to or greater in height than the mechanical equipment.

	12.51.110
	

	Non-single family residential Projects
	
	

	At least 10% of a non-residential development project located west of I-15 shall be landscaped, not including area within an abutting right-of-way
	12.51.070
	

	At least 15% of a non-residential development project located east of I-15 shall be landscaped, not including area within an abutting right-of-way.
	12.51.070
	

	At least 40% of a planned development, condominium, multiple-family project,assisted living facility, planned development overlay, or non-single-family residential development project shall be landscaped open space. 
· Open space and common areas shall include a minimum of one tree and two shrubs per dwelling unit.
	12.51.070
	

	Parking Lot Landscaping
	
	

	Every parking lot consisting of more than 10 spaces and 3,500 square feet shall contain, at a minimum, internal landscaped islands as follows:
· Multiple-family residential: 10% of total parking lot area.
· Office and commercial: 7% of total parking lot area.
· Industrial and warehouse: 5% of total parking lot area.

	12.51.070
	

	Every 6 required parking spaces = 2 shrubs and 1 deciduous tree for parking island
	12.51.070
	

	Internal landscaped islands shall contain a minimum of 25 square feet and shall have a minimum average width of at least 5 feet
islands shall be located: 
· To define major drives and access ways;
· To delineate ends of parking rows;
· At aisle intersections; and
· Within parking rows.

	
	

	Artificial plants or landscaping shall not be permitted in the required parking lot landscaped areas.

	12.51.070
	

	Public Street and Parkstrip Landscaping.
	
	

	Except for approved driveways and pedestrian walkways, landscaping shall be provided along public streets. 
	12.51.070
	

	landscaped areas shall be provided within the area adjacent and parallel to the frontage of a public street or highway to the depth shown, as measured from the back of curb:
· Freeway and Parrish Lane-Centerville Marketplace: 30 feet;
· Arterial or collector street: 15 feet; and
· Minor or local street: 10 feet
	12.51.070
	

	1 tree = for every 25 feet of public street frontage in a required landscaped area. 
	12.51.070
	

	The slope of any earth berm adjacent and parallel to public street right-of-way shall not exceed a vertical to horizontal ratio of one to two (1:2) and shall be treated with suitable ground cover to prevent soil erosion.
	12.51.070
	

	Artificial plants or landscaping shall not be permitted in the required public street frontage and parkstrip areas
	12.51.070
	



2 | Page


2 | Page

image4.svg
   


image1.png




image2.svg
  
.MsftOfcThm_Accent6_lumMod_50_Fill_v2 {
 fill:#275317; 
}

 


image3.png




image5.png
y o <

/\S

CENTERVILLE
12 UTAH 7





