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COMMERCIAL SUBDIVISION – PRELIMINARY PLAT COMPLETENESS REVIEW 





Commercial Subdivision - Defined
Commercial subdivision includes any commercial, industrial, or multifamily residential subdivision, or any combination thereof, as more particularly defined in CMC 15.01.040.

Commercial Subdivision - Approval Procedure
Commercial Subdivisions require a three-step review process including concept plat preliminary plat, and final plat review. Concept plats are reviewed and approved by the Planning Commission (with a public hearing). Preliminary plats are reviewed and approved by the Planning Commission (with a public hearing). Final plats are reviewed and approved by the City Council.

Commercial Subdivision – Preliminary Plat
A preliminary plat is required for all subdivisions. The preliminary plat minimizes changes and revisions that might otherwise occur on a final plat. It ensures compliance with the subdivision with City ordinances and regulations before the final plat is initiated.    

Commercial Subdivision – Preliminary Plat Completeness Review
The completeness review is a preliminary step conducted by the Community Development Director to determine if the preliminary plat application is complete and eligible for substantive review. If the application is not complete, the Community Development Director shall notify the applicant that the application is incomplete and provide information regarding deficiencies. No further action will be taken on incomplete applications. The applicant has 90 days from the date of City notice of application deficiencies to correct the deficiencies or the application will be considered withdrawn. Incomplete applications are not entitled to vested rights. Once an application is deemed complete, the Community Development Director will notify the applicant that the application is complete, and the application will be processed and reviewed for compliance with City ordinances and standards.

Commercial Subdivision – Approval by Planning Commission
The Planning Commission shall hold a public meeting to review proposed preliminary plats for commercial subdivisions. During the review, the Commission will ensure the plat complies with City code, State law, and all conditions of conceptual plat approval. If in compliance, the Commission may approve the preliminary plat. If not, the Commission may deny the plat, with reasonings. The Commission may also impose reasonable conditions or requirements to be met before final approval. 

Commercial Subdivision – Expiration 
Once preliminary plat approval has been granted, the applicant may apply for final plat approval. Preliminary plat approval shall expire and have no further force or effect if a complete application for final plat approval is not submitted within twelve (12) months from the date of approval of the preliminary plat. This time period may be extended for up to six (6) months for good cause shown if the applicant petitions the Planning Commission for an extension prior to the expiration date. Only one extension may be granted for each approved preliminary plat. In those cases where a subdivision is proposed to be developed in phases, preliminary plat approval for the remaining portions of the subdivision shall not be voided if a complete application for final plat approval for the first phase is submitted within twelve (12) months from the date of approval of the preliminary plat and subsequent phases are recorded in accordance with the approved phasing plan.






Commercial Subdivision – Preliminary Plat Completeness Checklist
The following application, information, fees, and documentation is required for preliminary plat application completeness review. 

Project Name: 
Date: 
TRACKING HISTORY:  
Application Submitted:  
· Completeness Checklist DRC Meeting (1): 
· Completeness Checklist DRC Meeting (2)
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	Application Requirement
	Code Reference
	Department
	Comments
	

	Complete Online Application Form
	
	Planning 
	
	

	Approved Conceptual Subdivision (Conceptual Plat) 
	15.03.015
	Planning 
	
	

	Owner of Affidavit signed by Owner OR Application Signed by Owner’s Agent with Authorization Form
	
	Planning/ Legal 
	
	

	Application Fees
	15.03.020 & Fee Schedule 18.030

	Planning 
	
	

	Professional Services Deposit
	15.03.020 & Fee Schedule 18.040 & 18.060
	Planning 
	
	

	Legal Description of entire property
	15.03.030
	Engineering 
	
	

	Proposed changes to existing zoning district boundaries or zoning classifications or conditional use permits
	
	Planning
	
	

	Title Report for all property within the subdivision (current within 30 days of submittal)
	15.03.030
	Legal
	
	

	Any agreements with adjacent property owners
	15.03.030
	Legal 
	
	

	ALTA Survey (containing information from Table A as required by the City Engineer)
	15.03.030 

	Engineering/ Legal
	
	

	Plan Set: 
	
	
	
	

	Plan Set will include the following: 
· Plat
· Cover sheet 
· Existing Conditions Inventory Sheet (Survey) 
· Site Plan 
· Utility Plan Sheet
	ECI 12.50
Grading and Drainage Sheet, Utility Sheet, site plan 15.05
	
	
	

	Plans shall be drawn at a scale no smaller than one inch equals 100 feet on 24" x 36" sheets

One electronic copy shall be submitted

3 paper copies shall be submitted at the time of compliance review 

Each Sheet should include the following: 
· Engineer Contact information 
· Name 
· Phone number
· Firm
· Address
· Page number
· Revision block
· Date of latest draft or revision.
· North Arrow
· Scale not smaller than 1”=100’
· Top of the drawing faces either north or west
	15.03.030 & 15.07.030(d)
	Planning
	
	

	Plat: 

	Proposed name of subdivision in bold
	15.03.030
	Planning
	If a PDO, please include “PDO” at the end of the name. 
	

	Signature block for:
· authorized parties
· property owners
· lienholders
	15.03.030
	Planning/ Legal
	Visit the city Details and Drawlings

	

	Blocks for signature:
· Planning Commission
· City Engineer
· City Attorney
· City Council (a signature line for the Mayor and an attestation by the City Recorder)
· Davis County Recorder in the lower right corner
	15.04.030
	Planning
	
	

	Owners dedication certificate and signature line for each property owner of record and
significant lienholders
	
	Legal
	
	

	Notary public's acknowledgment for each signature on the plat
	
	Legal
	
	

	Certification of the accuracy of the preliminary plat of the subdivision and any traverse to permanent survey monuments by a land surveyor registered to practice in the State of Utah. ( Registered land surveyor's "Certificate of Survey”)
	15.03.030
	Engineering
	
	

	The location and dimensions to the nearest existing bench mark or monument, and section line.
	15.03.030
	Engineering
	
	

	Depiction of the survey mathematical information( bearing and distances), and data necessary to locate all monuments and to locate and retrace all interior and exterior boundary lines: 
· straight lines
· central angle
· radius and arc length of curves
	15.04.030
	Engineering
	
	

	A correct metes and bounds description of all property included within the subdivision
	
	Engineering
	
	

	The boundary lines of all lots tied to public survey monuments in the project showing: 
· Bearings
· Distances
· Dimensions
· Square footage
· Orientation
· Topography
(lines shall be slightly heavier than street and lot lines)
	15.03.030
	Planning/ Engineering
	
	

	The streets in the project showing: 
· Location
· Widths
· Distance
· Dimensions
· Dedication ( private or public)
· Name
	15.03.030
	Planning/ Public Works/ Engineering
	
	

	The alleys in the project showing: 
· Location
· Widths
· Distance
· Dimensions
· Dedication ( private or public)
	15.03.030
	Planning/ Public Works/ Engineering
	
	

	The easements in the project showing: 
· Location
· Widths
· Distance
· Dimensions 
· Squar Footage
· Dedication ( private or public)
	15.03.030
	Planning/ Public Works/ Engineering
	
	

	All lots shall have at least:
· 10' wide front yard public utility easements
· at least two other 7' wide side or rear yard public utility easements 
	15.05.060(h)
	Planning/ Engineering
	
	

	The parks in the project showing:
· Location
· Widths
·  Dimensions 
· Squar Footage
· Dedication ( private or public)
	15.03.030
	Planning/ Public Works
	
	

	The open space in the project showing: 
· Location
· Widths
·  Dimensions 
· Squar Footage
· Dedication ( private or public)
	15.03.030
	Planning
	
	

	Depiction of block width. 
The minimum width of a block shall not be less than 250 feet measured from center line of street to center line of street.
	15.05.010
	Planning
	
	

	Depiction of block length. 
The maximum length of blocks shall be 1200 feet. In blocks over 800 feet in length, a dedicated public walkway through the block, at approximately the center of the block, may be required. Such walkways shall not be less than 10 feet in width unless otherwise approved by the City.
	15.05.010
	Planning
	
	

	Cover sheet: 
	
	
	
	

	Cover Page including the following: 
· Engineer Contact information 
· Name 
· Phone number
· Firm
· Address
· Page number
· Development Use
· Engineer Stamp 
· General Notes
· Civil Drawlings Index
· Vicinity Map
	15.05.060
	Planning
	
	

	Site Plan will include: 

	Depiction of all lots front, side, and rear yard setback lines.
	15.05.020
	Planning
	
	

	Depiction of all lots frontage.
	15.05.020
	Planning
	
	

	Depiction of all lots buildable area. 
The buildable area is the portion of a property located outside the required setback distances from the property lines
	15.05.020
	Planning
	
	

	Depiction of all proposed fences, retention walls, or landscaping walls greater than 4 ft
	12.55.110
	Planning/ Engineering
	
	

	A sheet showing all retaining walls details, including their height relative to proposed grades (when involves fences, walls, grade changes, or in the Hillside Overlay Zone)
	12.21.110
	Planning
	
	

	The subdivider shall submit a landscaping indicating how maintenance of the landscaping will be performed and by whom ( separate checklist is required)
	15.05.070 (a)
	Planning
	
	

	Subdivisions in the Hillside Overlay Zone shall comply with all landscaping provisions of the Zoning Code, including, but not limited to, provisions of CZC 12.42
	15.05.070 (b)
	Planning
	
	

	Location, dimensions, and labeling of other features such as: 
· irrigation facilities
· bridges
· railroad tracks
· buildings
· bicycle racks
· dumpsters
· trash cans
· fences/ retaining walls (with grading plan)
· signage
· mechanical equipment
	12.21
	Planning
	
	

	Depiction of all off street parking 
	12.52
	Planning/ Engineering
	
	

	Depiction of snow load zones
	11.01.130
	Public Works
	
	

	Depiction of proposed sidewalks
	10.06.020
	Public Works/ Engineering
	
	

	Depiction of proposed signage 
	12.54
	Planning/ Public Works
	
	

	Table of Development Standards: 
· Setbacks from all property lines 
· Impervious surface sq ft and %
· Square footage of building footprint
· Square footage of total building floor area
· Square footage of street rights of way
· Residential Units
· Commercial Units
· Structure heights
· Distance between buildings
· Parking number
· Density 
· Landscape buffering %
· Floor area
	12.21.110
	Planning
	
	

	A development schedule indicating the approximate date when construction or its stages can be expected to begin and be completed
	12.21.110
	Planning/ Engineering/ Public Works
	
	

	Construction Plans will include the following: 

	Title block located in lower right corner of sheet to include:
· Project title (subdivision, etc.)
· Specific type and location of work
· Name of engineer or firm preparing drawings with license number
· Utah Engineers stamp shall be required on all construction plans
· Date of Plans
	15.07.030 (d)
	Planning
	
	

	All drawings and/or prints shall be: 
· 24" x 36" (trim line)
·  2" border on top, bottom, and right sides
· 1.5" border on the left side
	15.07.030 (c)
	Engineering
	Once deemed complete, this will be requested to start compliance review
	

	Elevations referenced to U.S.G.S. datum
	15.07.030 (d)
	Engineering
	
	

	Stationing and elevations for profiles
	15.07.030 (d)
	
	
	

	All structures shall be designed in accordance with minimum requirements established by the City Standards and Specifications
	15.07.030 (f)
	Engineering
	Review the City Details and Drawings 1701822707_Centerville City - Standard Details (2023)-adopted.pdf

	

	Each set of plans shall be accompanied by a separate sheet of details for structures which are to be constructed
	15.07.030 (e)
	Engineering
	
	

	Easement Sheet will include the following: 

	Utility easements shall be provided within the subdivision as required for public utility purposes. 
	15.05.060(h)
	Public Works/ Engineering 
	
	

	All utilities shall be provided through underground service, except where existing utilities are already in place. 
	15.05.060 (a)
	Public Works/ Engineering 
	
	

	All underground utilities shall be installed prior to the installation of road base, surfacing, curbs, gutters and sidewalks. 
	15.05.060 (a)
	Public Works/ Engineering 
	
	

	If underground utilities are not installed prior to street surfacing sleeves shall be required.
	15.05.060 (a)
	Public Works/ Engineering 
	
	

	Utility Sheet: 

	Plans for all the street utilities shall be drawn on the same plans. All existing and proposed utilities including, but not limited to: 
· Sewer
· culinary water
· secondary water
· fire hydrants
· storm drains
· subsurface drains
· gas lines
· power lines
· communications lines
· cable television lines
· streetlights
	15.07.020 
	Public Works/ Engineering 
	
	

	All streets should conform to the width designated by the Master Street Plan wherever a subdivision is in an area for which a Master Street Plan has been adopted. For territory where the Master Street Plan does not designate a street, streets shall be provided as required by the subdivision plat approving authority. 
	15.05.030 (c)
	Public Works/ Engineering 
	
	

	Local streets shall approach an arterial or collector street at an angle of at least 85 degrees. Grades for streets shall be a minimum of 0.5% and a maximum of 12% for all streets except major and minor arterials which shall be 10% maximum.
	15.05.030 (e)
	Public Works/ Engineering 
	
	

	Dedication of half streets is prohibited unless: 
· a full right of way is to be obtained; curb, gutter, and sidewalk is constructed on the subdivider's side
· and a minimum of 28 feet of asphalt is laid. 
the balance of street improvements will be provided by the applicable property owner
	15.05.030 (b)
	Public Works/ Engineering 
	
	

	Cut and Fill Specifications
	15.05.030 & 15.05.070 
	Public Works/ Engineering 
	
	

	Curbs, gutters, and sidewalks shall be installed on existing and proposed streets by the applicant in all subdivisions.
	15.05.030 (d)
	Public Works/ Engineering 
	
	

	Both plan view and profiles for curb and gutter plans shall be shown for each side of the street; street center line profile may be eliminated. Top of curb elevations with curve data must be shown for all curb returns.
	15.07.030 (d)
	Public Works/ Engineering 
	
	

	Permanent monuments shall be furnished, accurately established, and set by the subdivider's surveyor at such points as are necessary to definitely establish all lines of the plat except those defining individual lots.
	15.05.030(i)
	Public Works/ Engineering 
	
	

	Protection Strips be shown to adhere to CMC 15.05.040 
	15.05.040
	Public Works/ Engineering 
	
	

	City shall furnish and install all required street signs and the cost thereof shall be charged to and paid by the subdivider in accordance with the City Fee Schedule 17.010
	15.05.030(h)
	Public Works/ Engineering 
	
	

	City approved street lights shall be depicted and installed at all:
· street intersections 
· school or pedestrian crossings
· bends or curves in the street at intervals 
	15.05.060(g) & 15.05.030(j) 
	Public Works
	
	

	Cul de sacs shall:
· serve no more than 20 lots or units
· be no longer than 400 feet, measured from the center point of the turn around to the center line of the intersecting street must be terminated with a turn around of not less than 100 feet in diameter
	15.05.030 (f)
	Public Works/ Engineering 
	
	

	Downhill cul de sacs are not permitted unless adequate drainage and 100 year over flow is provided 
	15.05.030 (f)
	Public Works/ Engineering 
	
	

	Where a street is designed to remain only temporarily as a dead end street, a satisfactory temporary turn-around area and recordable easement shall be provided at the end thereof to remain and be available for public use so long as the dead end exists. The City may require improvements to be installed in temporary turn-around areas.
	15.05.030 (g)
	Public Works/ Engineering 
	
	

	Proposed off site and on site fire hydrants.
	15.03.030
	SDFD/ Public Works
	
	

	Hydrants located within 350 feet of any building site in the subdivision shall be charged with water and must be operable before a building permit may be issued.
	15.05.060 (c)
	SDFD/ Public Works
	
	

	Fire hydrant spacing shall not exceed 400 feet.
	15.05.060 (c)
	SDFD/ Public Works
	
	

	Fire hydrants shall be installed by the City, at the subdivider's expense, at locations determined by the City Engineer and the Fire Department.
	15.05.060 (c)
	SDFD/ Public Works
	
	

	Utility Sheet Culinary Water requirements: 

	Proposed off site and on site culinary water. 
	15.03.030
	Public Works
	
	

	Size and location of culinary water lateral mains, meters, valves and hydrants (these plans to be finalized by the City Engineer).
	15.07.030 (d)
	Public Works/ Engineering 
	
	

	A culinary water supply, which must be approved by the City Engineer shall be available to each lot in the subdivision and shall be provided in conformance with the standards and rules and regulations of the City and requirements of the City Engineer. Where an approved public water supply is available, the City shall cause to be installed, at the subdivider's expense, water mains, valves, pressure reducing valves, and service laterals to each lot within the subdivision.
	15.05.060 (b)
	Public Works/ Engineering 
	
	

	Utility Sheet Secondary Water/ Irrigation requirements: 

	Proposed off site and on site secondary water facilities.
	15.03.030
	Public Works
	
	

	Secondary water for the purpose of irrigation shall be made available to each lot in all residential subdivisions
	15.05.060 (e)
	Public Works/ Engineering 
	
	

	Size and location of irrigation lateral mains, valves, fittings, etc.
	15.07.030 (d)
	Public Works/ Engineering 
	
	

	The applicable connection fee shall be paid to the irrigation district prior to their approval of the final plat.
	15.05.060 (e)
	Public Works/ Engineering 
	
	

	The subdivider will be required, at its own expense, to construct all required off site facilities to connect to existing irrigation district facilities. 
	15.05.060 (e)
	Public Works/ Engineering 
	
	

	The size of service connections allowed will be determined by the irrigation district. 
	15.05.060 (e)
	Public Works/ Engineering 
	
	

	Construction of irrigation water facilities shall be subject to the approval of the appropriate pressure irrigation district, as signified by its letter of approval.
	15.05.060 (e)
	Public Works/ Engineering 
	
	

	Utility Sheet Sanitary Sewer requirements: 

	Proposed off site and on site sanitary sewers.

	15.03.030
	Public Works
	
	

	The subdivider shall connect with a public sanitary sewer and provide sewer mains and extend laterals from the sewer main to each lot in the subdivision
	15.05.060 (d)
	Public Works/ Engineering 
	
	

	Size and location of sewer, storm drains, and subdrains, and manhole cleanouts
	15.07.030 (d)
	Public Works/ Engineering 
	
	

	Type of pipe.

	15.07.030 (d)
	Public Works/ Engineering 
	
	

	Utility Sheet Storm Drain requirements: 

	Proposed off site and on site storm drainage facilities
	15.03.030
	Public Works
	
	

	The use of any subsurface drains within a subdivision may be permitted on a limited basis, as deemed appropriate by the City, in accordance with the procedures and requirements set forth in CMC 9.06 (Subsurface Water) regarding subsurface drains, and shall require videotaping prior to final inspection in accordance with CMC 9.06.080. 
	15.05.060 (f)
	Public Works/ Engineering 
	
	

	All storm water drainage systems, improvements and facilities installed by the developer shall comply with applicable provisions of CMC 16 (Stormwater), and shall require videotaping prior to final inspection in accordance with City Fee Schedule.
	15.05.050(e)
	Public Works/ Engineering 
	
	

	The subdivider shall construct and install a storm water drainage system within the subdivision which shall be constructed of materials and according to the City Standards and Specifications and the requirements of the Storm Drainage Master Plan.
	15.05.050(a)
	Public Works/ Engineering 
	
	

	The storm water drainage system for subdivider's subdivision shall be connected to an approved off site storm drain or facility acceptable to the City.

	15.05.050(c)
	Public Works/ Engineering 
	
	

	The subdivider shall dedicate a right of way of 15 feet in width or greater as required by the City for storm drainage conforming substantially with the lines of any natural watercourse or channel, stream, creek, irrigation ditch, or floodplain that enters or traverses the subdivision as determined by Davis County Flood Control and/or the City Engineer. 
	15.05.050(b)
	Public Works/ Engineering 
	
	

	The subdivider shall dedicate rights of way for any pipe, conduit, channel, and retention or detention area as recommended by the City Engineer.
	15.05.050(b)
	Public Works/ Engineering 
	
	

	Storm drain, cross gutters, dipstone inlets, and other appurtenant structures shall be provided by the subdivider (within the limits of the subdivision) as required to adequately dispose of storm waters and the 10 year frequency storm flows developed within the limits of the subdivision and the existing flows entering the proposed subdivision from adjacent properties.
	15.05.050(d)
	Public Works/ Engineering 
	
	

	Approval of any Subsurface drains in accordance with applicable provisions and a copy of proposed protective covenants in all cases where subsurface drains are to be located within the subdivision, as applicable. 
	9.06
	Public Works/ Engineering 
	
	

	Contour Drainage Plans 
	Title 16 
	Public Works/ Engineering 
	
	

	Storm Water Maintenance Plan Submitted A tentative plan by which the subdivider proposes to handle storm water drainage for an event with a 10 year return interval, as determined by the City Engineer.

	15.03.030
Title 16 
	Public Works/ Engineering 
	
	

	Storm Water Maintenance Plan Agreement Signed 
	Title 16 
	Public Works/ Engineering 
	
	

	Additional City Code Requirements: 

	Existing Conditions Inventory (separate sheet)
	12.50.040
	
	Before a site plan or other development approval is reviewed and approved, an existing conditions inventory, as required. Please see list below. 
	

	Evidence that all utilities and services will be available for the subdivision and providers have been notified 
	15.03.030
	Planning
	· Lumin (Century Link & Quantum Fiber)
· Weber Basin Water District/Deuel Creek Irrigation Co
· Enbridge (Dominion Energy)
· Rocky Mountain Power
· South Davis Metro Fire
· South Davis Sewer District
· Utopia Fiber
· Xfinity Cable Service\
· Davis County Health Department 
· UDOT Region One (1)
	

	Submit a Land Scaping Plan designed by a Utah Certified Landscape Architect
	15.05.070
	Planning
	
	

	Explanation of RDA Request ( if applicable) 
	Requested- not required
	Community Development Director
	
	

	All lots or parcels created by the subdivision shall have frontage on a dedicated street, improved to standards equal to at least 50% of its minimum required width. 
	15.05.020(b)
	Planning
	
	

	"As builts" shall be provided by the developer and submitted to the City prior to final inspection. 
	15.05.060 (e)
	
	
	


Additional Staff Comments for Completeness:


Comment History:
	Completeness Checklist DRC Meeting (1): 
Please address the following items:
· Review the City Details and Drawings 1701822707_Centerville City - Standard Details (2023)-adopted.pdf
· 



	Completeness Checklist DRC Meeting (1): 
Please address the following items:
· 
· 




	Title
	Name
	Email 
	Phone

	Public Works Director
	Mike Carlson
	Mike.carlson@centervilleutah.gov 
	801-677-6093

	Deputy Public Works Director
	Dave Walker
	Dave.walker@centervilleutah.gov
	801-677-6099

	Drainage Supervisor
	Cameron Woodbury 
	cameron.woodbury@centervilleutah.gov
	801-677-6096

	Streets Supervisor
	Marc Marchant
	Marc.marchant@centervilleutah.gov
	801- 335- 8854

	Water Supervisor
	Steve Hunt
	Steven.hunt@centervilleutah.gov
	801-335- 8844

	Community Development Director
	Michael Eggett
	Michael.eggett@centervilleutah.gov
	801-677-6437

	City Planner
	Sydney DeWees
	Sydney.dewees@centervilleutah.gov
	801-677-6097

	City Attorney 
	Lisa Romney
	Lisa.romney@centervilleutah.gov
	801-335-8842

	City Engineer
	Kevin Campbell
	Kevin.campbell@esieng.com
	801- 953-4812

	South Davis Fire Marshal
	Cole Fessler
	cfessler@sdmetrofire.gov
	801-677-2400

	South Davis Fire Inspector 
	Travis Mander
	tmander@sdmetrofire.gov
	801-677-2400
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EXISTING CONDITIONS INVENTORY –






Existing Conditions Inventory - Defined
Existing Conditions Inventory includes plans that gather information about a development site prior to approval of a site plan or other development approval in order to avoid approving plans that create land use conflicts and to protect natural and cultural resources that may be adversely affected by construction activities.

Existing Conditions Inventory – Review Procedure
Before a site plan or other development approval is reviewed and approved, an existing conditions inventory, as required in CZC 12.50.040, shall be provided for the subject property and for the first 100 feet of adjoining property. ECI will be in conjunction with the ALTA Survey. Items in the ALTA will not be required on the ECI. If no ALTA is required, an separate ECI is required in the civil plans. 

Project Name: 
Date: 
TRACKING HISTORY:  
· Application Submitted:  
· Completeness Checklist DRC Meeting (1): 
· Completeness Checklist DRC Meeting (2):
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	Application Requirement
	Code Reference
	Department
	Comments
	

	Submitted on one or more 24” x 36” sheet
	12.50.040
	Planning
	
	111

	Depiction of streams drainage course.
	12.50.040
	Engineering
	
	112

	Depiction of floodplains located on or within 100 feet of the subject property.
	12.50.040
	Engineering
	
	113

	Floodplains shall be as delineated on Federal Emergency Management Agency (FEMA) flood insurance rate maps
	12.50.040
	Public Works- Drainage 
	
	114

	Floodplain elevations for a 100 year flood event shall be depicted by topographic delineation
	12.50.040
	Public Works- Drainage 
	
	115

	Depiction of the slope categories based on the City topographic maps: 
· 0-10%;
· 10-20%;
· 20-30%; and
· 30% or more.
	12.50.040
	Engineering
	
	116

	Depiction of sensitive soils (as identified on any soil survey prepared for a government body).
	12.50.040
	Engineering
	
	117

	Description of soil limitations on development
	12.50.040
	Engineering
	
	118

	Description of soils with severe limitation shall be noted separately
	12.50.040
	Engineering
	
	119

	Depiction of seasonal high water table
	12.50.040
	Engineering
	
	120

	Depiction of flood hazard
	12.50.040
	Public Works- Drainage/ Engineering
	
	121

	Depiction of poor drainage
	12.50.040
	Public Works- Drainage/ Engineering
	
	122

	Depiction of wetland/hydric soil conditions 
	12.50.040
	Engineering
	
	123

	Depiction of high shrink/swell potential
	12.50.040
	Engineering
	
	124

	Depiction of shallow depth to bedrock
	12.50.040
	Engineering
	
	125

	Depiction of excessive slopes
	12.50.040
	Engineering
	
	126

	Depiction of high susceptibility to erosion
	12.50.040
	Engineering
	
	127

	Depiction of wetlands which are required to be delineated by the Clean Water Act.
	12.50.040
	Public Works- Drainage/ Engineering
	
	128

	Depiction wetlands by a line denotating the boundaries
	12.50.040
	Public Works- Drainage/ Engineering
	
	129

	A copy of any application for authorization to impact or alter wetlands
	12.50.040
	Public Works- Drainage/ Engineering
	
	130

	Depiction of shrub and tree stands (as indicated by recent aerial photos)
	12.50.040
	Engineering
	
	131

	Depiction of the shrub and tree area by a circumferential line extending to the outer perimeter of the tree or shrub canopies
	12.50.040
	Engineering
	
	132

	Depiction of any existing utility line, aqueduct, dam, ditch, or canal located within the area subject to the ECI.
	12.50.040
	Engineering
	
	133

	Depiction of any area which may be flooded in the event an aqueduct, dam, ditch, or canal fails, as contained in any study conducted and/or possessed by the City or the Utah State Engineer
	12.50.040
	Engineering
	
	134

	Depiction of natural features on the site and within 500 feet of any portion of it 
	15.03.030
	Planning
	
	135

	Depiction of manmade features on the site and within 500 feet of any portion of it 
	15.03.030
	Planning
	
	136

	Depiction of areas identified as special protection areas in this Title, the General Plan, and other documents adopted by the City, including, but not limited to, wellhead protection areas and groundwater recharge areas
	12.50.040
	Planning/ Engineering
	
	137

	Depiction of cultural and historic resources, including cemeteries, identified in the General Plan
	12.50.040
	Planning
	
	138

	Note whether the property is located within a designated historic district.
	12.50.040
	Planning
	
	139

	Source of the ECI data
	12.50.040
	
	
	140

	If a factor is not applicable to the subject property, the ECI shall include a note to that effect.
	12.50.040
	
	
	141



Additional Staff Comments:
Please address the following items:
· 
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