CITY OF CLARKSBURG
INVITATION FOR BIDS
Salt Storage Building Construction Project
The City of Clarksburg Public Works Department is soliciting sealed bids from qualified contractors for the furnishing of labor, materials, equipment, transportation, supervision, and all incidentals necessary for the construction of a new salt storage building at the Public Works Facility.
The project consists of furnishing and installing concrete bin blocks, constructing a reinforced concrete floor slab, and supplying and erecting an engineered roof system. The City of Clarksburg Public Works Department will perform site grading, excavation of footers, and placement/compaction of crush-and-run base material prior to contractor mobilization.

Project Specifications
Salt Storage Building
The completed structure shall consist of:
· Approximately 40 feet wide x 40 feet deep 
· Engineered 40-foot x 40-foot x 13-foot double truss roof system 
· Open front design suitable for loading and unloading road salt 
· Concrete bin block containment walls 
· Reinforced concrete floor slab 

Scope of Work
1. Concrete Bin Block Supply and Installation
Contractor shall furnish, deliver, and install:
· Seventy-two (72) precast  6-foot concrete bin blocks 
· Eight (8) precast concrete corner blocks 
· Eight (8) precast concrete 3-foot bin blocks 
All blocks shall be properly aligned, leveled, interlocked, and secured to create the storage structure.

2. Reinforced Concrete Floor Slab
Contractor shall furnish and install:
· Approximately 65 cubic yards of 4,000 PSI concrete 
· Reinforcing steel 
· Welded wire reinforcement 
· Dowel bars drilled and epoxied into bin blocks 
· Formwork as required 
· Concrete placement and finishing 
· Saw-cut control joints 
· Joint sealing 
· Final curing and cleanup 
The slab shall be designed to withstand repeated loading from dump trucks, loaders, and other Public Works equipment.

3. Roof System
Contractor shall furnish, deliver, and erect:
· One (1) 40' x 40' x 13' engineered double truss roof system 
· Complete structural framing package 
· Roof panels and accessories 
· Anchoring system 
· All hardware and fasteners 
· Shop drawings and engineering certification 
The roof system shall be designed to meet all applicable West Virginia wind and snow load requirements.

Work by City of Clarksburg Public Works
The City will provide the following work prior to contractor mobilization:
· Site grading and leveling 
· Excavation of required footers 
· Placement of crush-and-run stone base 
· Compaction of crush-and-run stone 
· Access to the project site 
Contractors shall include only the work specifically outlined in the Scope of Work section of this bid package.

Contractor Responsibilities
The contractor shall provide:
· All labor 
· Equipment 
· Materials 
· Transportation 
· Supervision 
· Temporary safety measures 
· Insurance 
· Cleanup and debris removal 
The contractor shall verify all dimensions and field conditions before beginning work.

Bid Submission Requirements
Bidders shall provide:
1. Total Lump Sum Price 
2. Itemized Cost Breakdown: 
· Bin Block Supply & Installation 
· Concrete Work 
· Roof System Supply & Installation 
3. Estimated Project Schedule 
4. Proof of Insurance 
5. West Virginia Contractor License Information 
6. References for similar projects completed within the last five years 

Warranty
The successful bidder shall provide:
· One (1) year warranty on workmanship 
· Manufacturer warranties on all supplied materials 
· Structural warranty provided by the roof system manufacturer 

