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	Site Plan Amendment– Completeness Checklist 
The following application, information, fees, and documentation is required for a Site Plan Amendment application completeness review.
Project Name: 
Date: 
TRACKING HISTORY:  
Application Submitted:  
Completeness Checklist DRC Meeting (1): 
Completeness Checklist DRC Meeting (2)
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	Application Requirement
	Code Reference
	Department
	Comments
	

	Original approved plan set of the final site plan 
	Requested
	Planning
	
	

	Copy of the terms and conditions for approval
	Requested
	Planning
	
	

	Complete Online Application Form
	12.21.110 
	Planning 
	
	

	Application Fees
	20.130
	Planning 
	
	

	A current title report disclosing all recorded matters of title regarding the parcel which is prepared and dated not more than 30 days from the date of submittal of the application for permitted use permit.
	15.02.020& 12.21.110 
	Legal
	
	

	List of current owners of each property as indicated by current records of the Davis County Recorder’s Office.
	12.21.110 
	Planning 
	
	

	Provide a statement describing the proposed project. 
	12.21.110
	Planning 
	
	

	Copies of any agreements with adjacent property owners relevant to the proposed boundary line adjustment.
	12.21.110 
	Legal
	
	

	Signed Property Owner Affidavit
	12.21.110 
	Planning/ Legal
	
	

	A letter from providers, addressing the feasibility and their requirements to serve the project
	
	
	· Lumin (Century Link & Quantum Fiber)
· Weber Basin Water District/Deuel Creek Irrigation Co
· Enbridge (Dominion Energy)
· Rocky Mountain Power
· South Davis Metro Fire
· South Davis Sewer District
· Utopia Fiber
· Xfinity Cable Service\
· Davis County Health Department 
· UDOT Region One (1)
	

	Plan Set including: 
· Cover sheet 
· Existing Conditions Inventory Sheet (Survey)
· Site Plan 
· Grading and Drainage Sheet
· Utility Plan Sheet
· Building Elevation Sheet
	12.21.110 
	
	
	

	Site Plan 
	
	
	
	

	Plans shall be drawn at a scale no smaller than one inch equals 100 feet on 24" x 36" sheets

One electronic copy shall be submitted

3 paper copies shall be submitted at the time of compliance review 

Each Sheet should include the following: 
· Engineer Contact information 
· Name 
· Phone number
· Firm
· Address
· Page number
· North Arrow
· Scale
	12.21.110 
	Planning
	
	

	Site Plan Cover Page: 
	
	
	
	

	Cover Page including the following: 
· Engineer Contact information 
· Name 
· Phone number
· Firm
· Address
· Page number
· Development Use
· Engineer Stamp 
· Vicinity Map
	12.21.110 & 15.05.060
	Planning
	
	

	Site Plan Sheet

	Site address
	12.21.110 
	Planning
	
	

	Total acreage 
	12.21.110 
	Planning
	
	

	Tax identification number for the parcel
	12.21.110 
	Planning
	
	

	Legal description of the property and parcel number
	12.21.110 
	Planning
	
	

	Tie to a Section monument
	12.21.110 
	Engineering 
	
	

	The boundary lines of all lots in the project showing: 
· Bearings
· Distances
· Dimensions
· Square footage
· Orientation
· Topography
	12.21.110 
	Planning/ Engineering
	
	

	Subject property existing and proposed buildings: 
· Location
· Height
· Setbacks 
	12.21.110 
	Planning
	
	

	Relationship of the property to adjoining properties and uses for of existing and proposed buildings: 
· Location
· Height
· Setbacks 
	12.21.110 
	Planning
	
	

	Location, arrangement and layout of landscaping and open space (addental checklist is required) 
	12.21.110
	Planning
	
	

	Location, dimensions, and labeling of other features such as: 
· irrigation facilities
· bridges
· railroad tracks
· buildings
· bicycle racks
· dumpsters
· trash cans
· fences/ retaining walls (with grading plan)
· signage
· mechanical equipment
	12.21.110
	Planning
	
	

	A sheet showing all retaining walls details, including their height relative to proposed grades (when involves fences, walls, grade changes, or in the Hillside Overlay Zone)
	12.21.110
	Planning
	
	

	An elevation plan drawn to scale showing elevations of existing and proposed structures 
	12.21.110
	Planning
	
	

	Layout, dimensions, and names of existing and future road right-of-way, private street, and sidewalks 
	12.21.110
	Public Works
	
	

	Traffic circulation patterns
	12.21.110
	Engineering
	
	

	Pedestrian circulation patterns
	12.21.110
	Engineering
	
	

	Access to the property
	12.21.110
	Engineering/ Public Works 
	
	

	Final Parking Plan ( separate checklist)

	12.21.110
	Planning/ Public Works
	
	

	Proposed reservations for parks, playgrounds, school, and other public facility sites, if any;

	12.21.110
	Planning/ Public Works
	
	

	Table of Development Standards: 
· Setbacks from all property lines 
· Impervious surface sq ft and %
· Square footage of building footprint
· Square footage of total building floor area
· Square footage of street rights of way
· Residential Units
· Commercial Units
· Structure heights
· Distance between buildings
· Parking number
· Density 
· Landscape buffering %
· Floor area
	12.21.110
	Planning
	
	

	A development schedule indicating the approximate date when construction or its stages can be expected to begin and be completed
	12.21.110
	Planning/ Engineering/ Public Works
	
	

	Any existing easements, driveways, utilities and infrastructure improvements
	12.21.110
	Planning
	
	

	Existing Conditions Inventory/ Survey Sheet: 
	
	
	
	

	A topographical drawing prepared by a licensed surveyor or civil engineer, showing existing topography in dashed lines at two foot intervals (in the Hillside Overlay Zone) or 5 ft intervals in all other areas and showing the proposed grade in solid lines at two foot intervals structurers
	12.55.134 
	Planning
	
	

	Depiction of streams drainage course.
	12.50.040
	Engineering
	
	

	Depiction of floodplains located on or within 100 feet of the subject property.
	12.50.040
	Engineering
	
	

	Floodplains shall be as delineated on Federal Emergency Management Agency (FEMA) flood insurance rate maps
	12.50.040
	Public Works- Drainage 
	
	

	Floodplain elevations for a 100 year flood event shall be depicted by topographic delineation
	12.50.040
	Public Works- Drainage 
	
	

	Depiction of the slope categories based on the City topographic maps: 
· 0-10%;
· 10-20%;
· 20-30%; 
· 30% or more.
	12.50.040
	Engineering
	
	

	Depiction of sensitive soils (as identified on any soil survey prepared for a government body).
	12.50.040
	Engineering
	
	

	Description of soil limitations on development
	12.50.040
	Engineering
	
	

	Description of soils with severe limitation shall be noted separately
	12.50.040
	Engineering
	
	

	Depiction of seasonal high water table
	12.50.040
	Engineering
	
	

	Depiction of flood hazard
	12.50.040
	Public Works- Drainage/ Engineering
	
	

	Depiction of poor drainage
	12.50.040
	Public Works- Drainage/ Engineering
	
	

	Depiction of wetland/hydric soil conditions 
	12.50.040
	Engineering
	
	

	Depiction of high shrink/swell potential
	12.50.040
	Engineering
	
	

	Depiction of shallow depth to bedrock
	12.50.040
	Engineering
	
	

	Depiction of excessive slopes
	12.50.040
	Engineering
	
	

	Depiction of high susceptibility to erosion
	12.50.040
	Engineering
	
	

	Depiction of wetlands which are required to be delineated by the Clean Water Act.
	12.50.040
	Public Works- Drainage/ Engineering
	
	

	Depiction wetlands by a line denotating the boundaries
	12.50.040
	Public Works- Drainage/ Engineering
	
	

	A copy of any application for authorization to impact or alter wetlands
	12.50.040
	Public Works- Drainage/ Engineering
	
	

	Depiction of shrub and tree stands (as indicated by recent aerial photos)
	12.50.040
	Engineering
	
	

	Depiction of the shrub and tree area by a circumferential line extending to the outer perimeter of the tree or shrub canopies
	12.50.040
	Engineering
	
	

	Depiction of any existing utility line, aqueduct, dam, ditch, or canal located within the area subject to the ECI.
	12.50.040
	Engineering
	
	

	Depiction of any area which may be flooded in the event an aqueduct, dam, ditch, or canal fails, as contained in any study conducted and/or possessed by the City or the Utah State Engineer
	12.50.040
	Engineering
	
	

	Depiction of areas identified as special protection areas in this Title, the General Plan, and other documents adopted by the City, including, but not limited to, wellhead protection areas and groundwater recharge areas
	12.50.040
	Planning/ Engineering
	
	

	Depiction of cultural and historic resources, including cemeteries, identified in the General Plan
	12.50.040
	Planning
	
	

	Note whether the property is located within a designated historic district.
	12.50.040
	Planning
	
	

	Source of the ECI data
	12.50.040
	
	
	

	If a factor is not applicable to the subject property, the ECI shall include a note to that effect.
	12.50.040
	
	
	

	Grading and Drainage Sheet: 
	
	
	
	

	Topography contours at 2-foot intervals
	12.21.110
	Public Works/ Engineering 
	
	

	Areas of substantial earth moving with an erosion control plan
	12.21.110
	Public Works/ Engineering 
	
	

	Storm Water Maintenance Plan Submitted 
	Title 16 
	Public Works/ Engineering 
	
	

	Storm Water Maintenance Plan Agreement Signed 
	Title 16 
	
	
	

	Location of existing:
· water course
· canals
· ditches
· springs
· wells
· culverts
·  storm drains
	12.21.110 & Title 16 
	Public Works/ Engineering 
	
	

	Location of any designated floodplain and/or wetland boundaries
	12.21.110 & Title 16 
	Public Works/ Engineering 
	
	

	Direction of: 
· storm water flows
· catch basins
· inlets
· outlets
· waterways
· culverts
· detention basins
· orifice plates
· outlets to off-site facilities
· off-site drainage 
	12.21.110
	Public Works/ Engineering 
	
	

	Utility Plan Sheet:
	
	
	
	

	All existing and proposed utilities including, but not limited to: 
· Sewer
· culinary water
· secondary water
· fire hydrants
· storm drains
· subsurface drains
· gas lines
· power lines
· communications lines
· cable television lines
· streetlights
	12.21.110
	Public Works/ Engineering 
	
	

	Minimum fire flow required by the Construction Codes for the proposed structures, and fire flow calculations at all hydrant locations
	12.21.110
	Public Works/ Engineering 
	
	

	Contour Drainage Plans 
	Title 16 
	Public Works/ Engineering 
	
	

	Cut and Fill Specifications
	15.05.030 & 15.05.070 
	Public Works/ Engineering 
	
	

	Where one or more conditions of unusual soil, vegetation, geology or slope exist, resulting in increased fire, flood or erosion hazards, traffic circulation problems, sewage disposal problems, and potential property damage from extensive soil slippage and subsidence, an applicant shall, upon request of the Planning Commission or City Engineer, provide contour and drainage plans, cut and fill specifications, and soil and geologic reports. The required details of such reports and plans may vary depending on the severity of the unusual conditions, but in any event such plans and reports shall be reviewed and approved by the City prior to final approval of a development project.
	12.21.110
	Public Works/ Engineering 
	
	

	Location and dimensions of all utility easements
	12.21.110
	Public Works/ Engineering 
	
	

	Building Elevations Sheet: 
	
	
	
	

	Accurate front, rear, and side elevations drawn to scale
	12.21.110
	Planning 
	
	

	Exterior surfacing materials and colors, including roofing material and color
	12.21.110
	Planning 
	
	

	Outdoor lighting, furnishings, and architectural accents
	12.21.110
	Planning 
	
	

	Location and dimensions of signs proposed to be attached to the buildings or structure
	12.21.110
	Planning 
	
	



Alteration or expansion of an approved site plan may be permitted by the Zoning Administrator upon making the following findings:
1. The proposed amendment does not relate to a matter specifically required as a condition of approval by the approving authority;
2. Any proposed change of use is consistent with uses permitted on the site;
3. Existing uses were permitted when the site plan was approved, or have received a conditional use permit;
4. The proposed use and site will conform to applicable requirements of the Centerville Municipal Code;
5. The proposed alteration or expansion meets the approval standards of Subsection (f);
6. The architecture of the proposed alteration or expansion, and landscaping, site design and parking layout are compatible with facilities existing on the site; and
7. The site can accommodate any change in the number of employees on the site or any change in impact on surrounding infrastructure.

If the Zoning Administrator cannot make the findings required in the foregoing Subsection, a conditional use permit or amended site plan, as the case may be, shall be approved by the Planning Commission before any alteration or expansion occurs.
Following the Planning Commission meeting, a notice of decision shall be sent to the applicant, which notice shall include:
1. Decision
If approved,
2. Conditions of approval
3. Findings that support the approval 
If denied, 
2.   Findings that support the denial 
	      If tabled, 
	       2.   Reasoning for tabling the decision
                    3.   Date of next meeting
Any person adversely affected by a final decision of the Planning Commission regarding the transfer, issuance, revocation or denial of a conditional use permit may appeal that decision to the Board of Adjustment as provided in CZC 12.21.200.
A site plan amendment approval shall expire and have no further force or effect if the building, activity, construction or occupancy authorized by the approval is not commenced within one year or not substantially completed within two years from the date of final site plan approval.
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